; Any lines which start with a semi-colon will be ignored
; Blank lines signify the end of a section
; However the first non-commented line must be like below
; where the device name is OXFW911, OXFW900 or OXUF922
Configuration information for OXFW971

[hardware_config]
Audio_Core_Config 202f100a
DAC_Config 00000001
 
[1394.bus_info]
bus_dependent_info 20ff5003
Vendor_ID 0030e0
Chip_ID_Hi 02
Chip_ID_Lo 454647
 
[1394.root]
;Node_Capabilities 0083c0
Model_Number 00f971
 
[1394.unitAVC]
;Unit_Spec_ID 00a02d
;Software_Version 010001
Model_Number 00f971
 
[vendor_name]
"Oxford Semiconductor Ltd."
 
[device_type]
"OXFW 971"
 
[master_name]
"OXFORD Firewire speakers "
  
[AVC]
  
[1394.audioSubunitDescriptor]
Number_Of_Channels 8
; Channel_Config: Which channels are active in the cluster.The number of active channels
;                 must equal  Number_Of_Channels
;
;                 Any of the following fields ar permitted :
;                 LeftFront RightFront CentreFront LowFrequencyEnhancement LeftSurround RightSurround 
;                 LeftOfCentre RightOfCentre Surround SideLeft SideRight Top Bottom LeftFrontEffect
;                 RightFrontEffect 
;
; OR
;                 NonConventionalOrdering
Channel_Config LeftFront RightFront CentreFront LowFrequencyEnhancement LeftSurround RightSurround LeftOfCentre RightOfCentre
