This is a help file which gives details about the configuration of the uploader using
the settings avaiable in the file win_uploader.ini

Some of the information in the win_uploader.ini file is saved by the application when
it exits and is used so that the application can use this information the next time
it is executed. You will not ever have to edit these sections of the ini file. They are
labelled as automatic below.

Each line of the ini file starts with a text string and the information used is always
preceded by a colon. Here is a description of each of the lines

Unknown type is:
	Automatic
	
Add config offset address to firmware before uploading:
	0  - Don't add configuration information address for 1394 or USB
	1  - Add configuration information address for 1394 only
	2  - Add configuration information address for USB only
	3  - Add configuration information address for 1394 and USB
	>3 - Attempt to add configuration information addresses but carry on regardless
	
Wait before programming in secs:
	Time to wait after chip erase before starting to program the flash
	
Last flash index used:
	Automatic
	
Last configuration Information file:
	Automatic
	
Last firmware binary file:
	Automatic
	
Use SBP3 entries in unit directory:
	Automatic
	
Mode of operation:
	Add strings here separated by spaces which turn particular modes on
	FlashAdd - Enables the Add Flash button which allows the user to add flash devices to the database
	WriteImage - Enables the Write Image button to write an image of the flash to a file
Cloner Auto Inc :
	Automatic